The LF ATV Main Technical Specifications

	LF50ST-A Main technical specification

Size(length×width×height):1260mm×810mm×860mm

Wheel Base: 900mm

Track: 580mm

Minimum Ground Clearance: 130mm

Dead Weight: 110kg

Engine Type: single-cylinder, four-stroke, air-cooled, Reverse (single-cylinder, forced-air-cooled, four-stroke)

Engine Model: 1p39FMB (1P39QMB)

Bore × Stroke: 39mm×41.4mm

Displacement: 49ml (49.5ml)

Max. Power: 2.0kw/7500r/min (2.2kw/7500r/min)

Max. Torque: 2.5N.m/5000r/min (2.6N.m/6000r/min)

Clutch: Dry-type, auto centrifugal

Lubrication: pressure/ Splash

Start: Electric start/ kick start

Ignition: CDI

Maximum speed: 40km/h

Front Type Size and Air Pressure: 16×8-7

Rear Type Size and Air Pressure: 16×8-7

Start Performance: ≤15s

Brake Performance: ≤7m/30km/h

LF50ST-A, 610.00 USD/UNIT, FOB Chongqing Port.
	LF100ST-A Main technical specification

Size(length×width×height):1260mm×810mm×860mm

Wheel Base: 900mm

Track: 580mm

Minimum Ground Clearance: 130mm

Dead Weight: 110kg

Engine Type: single-cylinder, four-stroke, air-cooled, Reverse 

Engine Model: 1p50FMG-H

Bore × Stroke: 50mm×49.5mm

Displacement: 97ml

Max. Power: 4.5kw/7500r/min 

Max. Torque: 6.2N.m/5000r/min 

Clutch: Wet multi-plate

Lubrication: Pressure/ Splash

Start: Electric start

Ignition: CDI

Maximum speed: 40km/h

Front Type Size and Air Pressure: 16×8-7

Rear Type Size and Air Pressure: 16×8-7

Start Performance: ≤15s

Brake Performance: ≤7m/30km/h

LF50ST-A, 630.00 USD/UNIT, FOB Chongqing Port.

	LF125ST-A Main technical specification

Size(length×width×height):1480mm×890mm×910mm

Wheel Base: 985mm

Track: 665mm

Minimum Ground Clearance: 140mm

Dead Weight: 115kg

Engine Type: single-cylinder, four-stroke, air-cooled, Reverse 

Engine Model: 1P52FQMI 

Bore × Stroke: 52.4mm×57.8mm

Displacement: 124.65ml

Max. Power: 6.0kw/7000r/min 

Max. Torque: 7.65N.m/5000r/min 

Clutch: Dry-type, auto centrifugal

Lubrication: Pressure/ Splash

Start: Electric start/ Kick start

Ignition: CDI

Maximum speed: 40km/h

Front Type Size and Air Pressure: 19×7-8

Rear Type Size and Air Pressure: 18×9.5-8

Start Performance: ≤15s

Brake Performance: ≤7m/30km/h

LF50ST-A, 720.00 USD/UNIT, FOB Chongqing Port
	LF150ST-A Main technical specification

Size(length×width×height):1480mm×890mm×910mm

Wheel Base: 985mm

Track: 665mm

Minimum Ground Clearance: 140mm

Dead Weight: 115kg

Engine Type: single-cylinder, four-stroke, air-cooled, Reverse 

Engine Model: 1P57FQMJ 

Bore × Stroke: 57.4mm×57.8mm

Displacement: 149.6ml

Max. Power: 7.2kw/7500r/min 

Max. Torque: 9.0N.m/5500r/min 

Clutch: Dry-type, auto centrifugal

Lubrication: Pressure/ Splash

Start: Electric start/ Kick start

Ignition: CDI

Maximum speed: 40km/h

Front Type Size and Air Pressure: 19×7-8

Rear Type Size and Air Pressure: 18×9.5-8

Start Performance: ≤15s

Brake Performance: ≤7m/30km/h

LF50ST-A, 750.00 USD/UNIT, FOB Chongqing Port

	JS 250 ATV Main Technical Data

Size(length×width×height):1940mm×1005mm×1118mm

Minimum Ground Clearance: 115mm

Wheel Base: 1170mm

Basic weight (with oil and fuel): 215kg

Engine Type: single-cylinder, four-stroke, air-cooled, Reverse 

Displacement: 229.6cc

Primary reduction system: spur gear

Secondary reduction system: shaft drive

Transmission: Constant mesh.5 speed

Start: Electric start/ Kick start

Clutch: Wet multi-plate

Fuel tank capacity: 12L

Rear Tire: AT22×10-10

Front Tire: AT22×7-10

Front Suspension: strut

Rear Suspension: swing arm (monocross suspension)

Front Brake: drum brake

Rear brake: drum brake (full sealed)

JS 250 ATV, 1930.00 USD/UNIT, FOB Chongqing Port
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JS 250 ATV, 1950.00 USD/UNIT, FOB Chongqing Port

One 40ft can be load into: 32 units
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LF50ST, 610.00 USD/UNIT, FOB Chongqing Port.

One 40ft high container: 72 units.
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LF100ST-A, 630.00 USD/UNIT, FOB Chongqing Port

One 40ft high container: 52 units..

	[image: image4.jpg]



LF125ST, 720.00 USD/UNIT, FOB Chongqing Port

One 40ft container: 45 units.
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LF150ST, LF50ST-A, 750.00 USD/UNIT, FOB Chongqing Port.

One 40ft container: 45units.

	If you are interested in above ATV, kindly please contact Ms.Long Email: wlwang@cq114.com.cn or longli263@hotmail.com


